

|  |  |  |  |
| --- | --- | --- | --- |
| Model | **PL 170** | **PL 260** | **PL 260 M** |
| Loading pr. sequence | 80 litres | 120 litres | 160 litres |
| Cooling capacity, ice contents | 170 litres | 260 litres | 260 litres |
| Cooling capacity without ice bank | 27 litres /h | 43 litres /h | 43 litres /h |
| Pump capacity | 170 litres/h | 260 litres/h | 260 litres/h |
| Water surface | 0,4 m2 | 0,7 m2 | 1,0 m2 |
| Physical dimension LxWxH | 1300x700x  960mm | 2000x700x  960mm | 2500x700x  960mm |
| Weight net | 240 kg | 290 kg | 310 kg |
| Water quantity | 260 litres | 500 litres | 650 litres |
| Power supply | 230/1/50 | 230/1/50 | 230/1/50 |
| Power consumption | 1,5 Kw | 2,5 Kw | 2,5 Kw |
| Fuses | 10 amp | 16 amp | 16 amp |

Cooling capacity is designed on cooling of water from 70 °C to 3 °C.

* All SOVINOX models have user friendly and perfect working-height. Space for products on top.
* All SOVINOX models have special strong castors, which makes it easy to move.
* All SOVINOX models have a simple and user friendly panel in English language.
* All SOVINOX models are made so that maintenance can be easily carried out.
* All SOVINOX models are made in stainless steel with effective insulation and condensing protection.
* All SOVINOX models have cooling unit with approved, environmental cooling medium.
* All SOVINOX models are more efficient than other similar products we know.
* All SOVINOX models are produced in Norway and CE-approved.